{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[[2,3,3,3],[5,3,7,3],[8,3,9,3],[10,3,11,3],[12,3,13,3],[19,3,21,3],[22,3,23,3],[37,3,38,3],[5,4,7,4],[8,4,9,4],[10,4,11,4],[12,4,13,4],[22,4,23,4],[37,4,38,4]]}
["引脚脚号","引脚名称","功能名称","端口类型","说明","控制逻辑","备注"]
[24,"PA1","FAN2_PWM","PWM","负压风机PWM控制"]
[25,"PA2","OTH_UART2_TX","485-0"]
[26,"PA3","OTH_UART2_RX"]
[29,"PA4","KM_SPI_CSN","O"]
[30,"PA5","KM_SPI_SCK","SPI1","电机通讯"]
[31,"PA6","KM_SPI_SDO"]
[32,"PA7","KM_SPI_SDI"]
[68,"PA9","OTH_UART1_TX","UART1","调试"]
[69,"PA10","OTH_UART1_RX"]
[70,"PA11","OTH_CAN_RX","CAN1","与主控通讯"]
[71,"PA12","OTH_CAN_TX"]
[72,"PA13","OTH_SWDIO","SYS_DEBUG","SW模式下载"]
[76,"PA14","OTH_SWCLK"]
[35,"PB0","LED1","O","照明灯1","低有效"]
[36,"PB1","LED2","O","照明灯2","低有效"]
[37,"PB2","TEMP","I/O","配电箱温度计"]
[89,"PB3","FAN1_PWM","PWM","整机散热风扇1、2的PWM控制"]
[90,"PB4","PUMP","O","清洗泵控制"]
[91,"PB5","DOOR_INT0","I","关门光电，0位光电"]
[92,"PB6","DOOR_INT1",null,"限位光电"]
[93,"PB7","DOOR_INT2",null,"预留限位光电"]
[47,"PB10","OTH_UART3_TX","485-1","冷凝模块使用"]
[48,"PB11","OTH_UART3_RX"]
[95,"PB8","DOOR_INT3","I","开门按键"]
[96,"PB9","Alarm","O","声光电报警"]
[51,"PB12","KM_DIAG1","I","运动控制器的位置比较或DIR输出\n(SD_MODE = 0, SPI_MODE = 1)"]
[52,"PB13","KM_DIAG0","I","运动控制器的中断或STEP输出\n(SD_MODE=0，SPI_MODE = 1)"]
[15,"PC0","KM_REFL","O",null,null,{"$f":"_xlfn.DISPIMG(\"ID_462654F973254F94AABE2977EA77B377\",1)","v":"=DISPIMG(\"ID_462654F973254F94AABE2977EA77B377\",1)"}]
[16,"PC1","KM_REFR","O",null,null,{"$f":"_xlfn.DISPIMG(\"ID_976ADD971DDE4289B74AE081844CD38C\",1)","v":"=DISPIMG(\"ID_976ADD971DDE4289B74AE081844CD38C\",1)"}]
[18,"PC3","FAN0_POWER","O","底部散热风扇1、2电源","高电平打开"]
[33,"PC4","FAN1_POWER","O","整机散热风扇1、2电源","高电平打开"]
[34,"PC5","FAN2_POWER","O","负压风机电源","高电平打开"]
[63,"PC6","FAN0_PWM","PWM","底部散热风扇1、2的PWM输出"]
[64,"PC7","FAN0_FB_INT","I","底部散热风扇1反馈计数"]
[65,"PC8","FAN1_FB_INT","I","底部散热风扇2反馈计数"]
[66,"PC9","FAN2_FB_INT","I","整机散热风扇1反馈计数"]
[78,"PC10","OTH_UART4_TX","485-2","PH计使用"]
[79,"PC11","OTH_UART4_RX"]
[80,"PC12","FAN3_FB_INT","I","整机散热风扇2反馈计数"]
[7,"PC13","FAN4_FB_INT","I","负压风机反馈计数"]
[81,"PD0","WaterLevel_INT1","I","液位检测1","低有效"]
[82,"PD1","WaterLevel_INT2","I","液位检测2","低有效"]
[83,"PD2","WaterLevel_INT3","I","液位检测3","低有效"]
[84,"PD3","WaterLevel_INT4","I","液位检测4","低有效"]
[85,"PD4","WaterLevel_INT5","I","液位检测5","低有效"]
[86,"PD5","WaterLevel_INT6","I","液位检测6","低有效"]
[87,"PD6","WaterLevel_INT7","I","液位检测7","低有效"]
[88,"PD7","WaterLevel_INT8","I","液位检测8","低有效"]
[55,"PD8","WaterLevel_INT9","I","液位检测9","低有效"]
[56,"PD9","WaterLevel_INT10","I","液位检测10","低有效"]
[57,"PD10","WaterLevel_INT11","I","液位检测11","低有效"]
[58,"PD11","WaterLevel_INT12","I","液位检测12","低有效"]
[39,"PE8","OTH_DBG_LED1","O","设备运行状态debug灯","低有效"]
[45,"PE14","KM_EN","O","ENABLE PIN AND CONFIGURATION OF STANDSTILL POWER DOWN（5130）","高电平关闭"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}