{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["主键H","PA11"]
["主键M","PA16"]
["LED0","PA3"]
["LED1","PB13"]
["LED2","PA5"]
["LED3","PA6"]
["LED_R","PA7"]
["LED_G","PA8"]
["LED_B","PA9"]
["PWM","PA4"]
["风扇","PB1"]
["主键L"]
["主键K"]